| AUDIO XTRA HELP: ERROR CODES |
| The following is a list of error codes returned by Audio Xtra. It is important to notice that negative error codes are not Audio Xtra errors, but Director standard error codes.
0 | No error
-8219 | Unable to get file path. File not found.
-8220 | Invalid file operators
-8221 | File not found
-8222 | File positioning problem
-8223 | Disk is full
-8224 | File permission. Device in use.
-8225 | Out of file handles. Current record settings may not be supported by the installed audio driver.
-8226 | Misc. file error
-8227 | File already exists
-8228 | Lost network connection
-8229 | File is not open
-8230 | Chunk not found
-8231 | Invalid swap record
-8232 | At end of file
-8233 | Bad chunk size
-8234 | Drive not found
-8235 | File path is too long
-8236 | Invalid directory
-8700 | Out of memory
-8701 | Bad sound name
-8702 | Bad data type
-8703 | Misc. sound error
-8704 | Bad sound type
-8705 | Invalid member type
-8706 | Bad info type
-8707 | Duplicate sound name
-8708 | MIX services unavailable
-8709 | Cannot read this file format
-8710 | File format not supported
-8711 | Cannot set this
-8712 | No platform support
-8713 | No Shockwave permission
-8714 | Bad number of arguments
-8715 | Value out of range
-8716 | Too much hard drive space
-8717 | Cannot show Shockwave permissions
-8718 | This feature is not supported in Shockwave
-8719 | No private directory has been specified
-8720 | Invalid file path (contains path delimiters)
-8721 | Device not found
-8724 | unable to open mixer
-8725 | Unable to get mixer information
-8726 | No wave input devices
-8727 | Cannot control volume for this device
-8728 | Cannot control meter level for this device
-8729 | Misc. mixer error
-8730 | This is a mono device (used when trying to set/get the right volume)
-8731 | Mixer is unable to select a device
-8800 | Sound recorder closed
-8801 | Sound recording device in use
-8802 | Sound recorder busy
-8803 | Invalid sample rate
-8804 | Invalid sample depth
-8805 | Invalid compression type
-8806 | Input source string not found
-8807 | Input source type not found
-8808 | Sound hardware error
-8809 | No sound is recording
-8810 | Zero length sound recording
-8811 | Invalid file format
-8812 | Recorder already opened
-8813 | Zero-length recording buffer
-8814 | No sound input device available for recording. Verify that the sound card is functioning and its driver is installed.
-8815 | Invalid number of channels.
-8816 | Invalid sound format settings.
-8817 | RAM buffer exceeded.
-8818 | Recording is not paused (tried to call resume)
-8819 | Recording is already paused (tried to call pause)
-8820 | RAM recording buffer is full
-8821 | Invalid file extension for platform
-8900 | Sound already playing
-8901 | Sound not playing
-8902 | No sounds in list
-8903 | Zero length sound
-8904 | No free sound channels
-8905 | Bad sound format data
-8906 | Can not delete: sound is busy
-8950 | Width out of range (min = 4, max = 3096)
-8951 | Height out of range (min = 4, max = 255)
-8952 | Sound length is zero
-8953 | Sample frames are zero
-8954 | Channel is out of range (must be at least 1, max is # of channels in the sound)
-8955 | Plot buffer size is zero
-8956 | Plot buffer size not correctly divisible
-8957 | Plot buffer size too small
-8958 | Plot resolution is not one of the valid symbols (#low,#medium,#high,#maximum)
-8959 | Resolution too high for the width specified Will happen, if, for example, you try to plot a 100 ms sound over a width of 3000 pixels -- not enough sound data for this. Try #maximum if you get this or else decrease the width of the bitmap
-9000 to -9404 -9406 on | Internal Audio Xtra error code. Should never be returned. Contact support with the name of the function that produced the error.